# 0456p SAFETYLINE JALOUSIE louvre windows

Branded worksection

This branded worksection *Template* has been developed by NATSPEC in conjunction with **Safetyline Jalousie** (the Product Partner) louvre windows and may be used whilst the Product Partner is licensed to distribute it. The copyright remains with NATSPEC. As with all NATSPEC worksections, it is the responsibility of the user to make sure it is completed appropriately for the project. The user should also review its applicability for local conditions and regulations. Check [www.natspec.com.au](http://www.natspec.com.au/) for the latest updated version.

Worksection abstract

This branded worksection *Template* is applicable to Safetyline Jalousie louvre windows manufactured by SMR Designs Pty Ltd supplied as complete systems, and including installation accessories, such as fixings, flashings, sealants, joint sealing and weather-stripping, necessary for the satisfactory functioning of the whole.

How to use this worksection

This worksection *Template* must be customised for each project. See [A guide to NATSPEC worksections](https://www.natspec.com.au/a-guide-to-natspec-worksections) ([www.natspec.com.au](https://www.natspec.com.au/a-guide-to-natspec-worksections)) for information on *Template* structure, word styles, and completing a worksection.

Related material located elsewhere in NATSPEC

If a listed worksection is not part of your subscription package and you wish to purchase it, contact NATSPEC.

Related material may be found in other worksections. See for example:

* *0432 Curtain walls* if the project contains windows and window-and-spandrel assemblies in addition to louvred windows.
* *0451 Windows and glazed doors* if the project contains windows other than to louvre windows.
* *0461 Glazing* for types of glass.
* *0462 Structural silicone glazing* for adhesive fixed glazing*.*
* *0463 Glass blockwork* if the project contains glass blockwork in addition to louvred windows.
* *0524 Partitions – glazed* for glazed internal partitions.

Material not provided in Product Partner

This worksection *Template* includes generic material which may not be provided by Safetyline Jalousie, including:

* Bushfire screens.
* Security window grilles.
* Frameless glass louvres. See the *Louvre windows* worksection.

Documenting this and related work

You may document this and related work as follows:

* Schedule windows on drawings to your office documentation policy.
* If documenting louvre windows in the *0451 Windows and glazed doors* worksection, delete this worksection.
* See NATSPEC TECHnote PRO 006 for glass types used in buildings.
* In bushfire-prone areas, document bushfire protection requirements to AS 3959 and the NCC. If documenting bushfire shutters, see AS 3959 clause 3.7 and *0457 External screens*.
* For information on the Window Energy Rating Scheme (WERS), see [www.wers.net](http://www.wers.net/).
* For information on the Australian Glass and Window Association (AGWA) Accreditation Program, see [www.agwa.com.au](https://www.agwa.com.au/).

The *Normal* style text of this worksection may refer to items as being documented elsewhere in the contract documentation. Make sure they are documented.

Search [acumen.architecture.com.au](http://acumen.architecture.com.au/), the Australian Institute of Architect's practice advisory subscription service, for notes on the following:

* Guarantees and warranties.
* Protection of openable windows.
* Daylighting of buildings.
* Revisiting energy efficiency in commercial buildings.

Specifying ESD

The following may be specified by retaining default text:

* Louvre assemblies for natural ventilation.
* Window seals to minimise air leakage when louvres shut.

The following may be specified using included options:

* Thermal performance to reduce heating/cooling load by specifying the required Total system U-Value, Total system SHGC, frame material (e.g. metal has higher conductivity than timber).
* Glass and frame selection with an acceptable Visible transmittance for natural lighting.
* High performance glass, e.g. low-e.

The following may be specified by including additional text:

* Re-use of salvaged louvres.
* Recycled material content, e.g. aluminium frames.

Refer to the NATSPEC TECHreport TR 01 on specifying ESD.

## General

SAFTEYLINE JALOUSIE LOUVRE WINDOWS PROFILE

Safetyline Jalousie is a leading louvre window brand with a history of more than 50 years in Europe. Since its arrival in the Australian market in 2009 Safetyline Jalousie has quickly established itself as high quality option for building specifiers looking for a louvre window system that delivers wide louvre spans (up to 1.4 m), impenetrable building security and weatherproof seals. Safetyline Jalousie is distributed by SMR Designs who have been involved in the Australian home improvement and commercial building market for more than 30 years with its other external louvre product Vergola.

### Responsibilities

#### General

Requirement: Provide Safetyline Jalousie louvre windows, as documented.

*Documented* is defined in *0171 General requirements* as meaning contained in the contract documents.

### Company contacts

#### Safetyline Jalousie technical contacts

Website: [www.safetylinejalousie.com.au/contact](http://www.safetylinejalousie.com.au/contact-us.html)

### Cross references

#### General

Requirement: Conform to the following:

* *0171 General requirements*.

*0171 General requirements* contains umbrella requirements for all building and services worksections.

List the worksections cross referenced by this worksection. *0171 General requirements* references the *018 Common requirements* subgroup of worksections. It is not necessary to repeat them here. However, you may also wish to direct the contractor to other worksections where there may be work that is closely associated with this work.

NATSPEC uses generic worksection titles, whether or not there are branded equivalents. If you use a branded worksection, change the cross reference here.

### Standards

#### General

Selection and installation: To AS 2047.

AS 2047 does not cover fixed louvres.

Building classification:

To use AS 2047, the building class needs to be nominated as follows:

* Housing: BCA Class 1 and 10.
* Residential: BCA Class 2, 3 and 4.
* Commercial: BCA Class 5, 6, 7, 8 and 9.

#### Glazing

Glass type and thickness: To AS 1288, if no glass type or thickness is nominated.

For glass type and thickness refer to AS 1288 Table 4.1 and to AS/NZS 4667.

Glass thickness may be governed by human safety and other requirements – see AS 1288 Sections 5. The commonly available thicknesses of various glasses are shown on the wind pressure figures of AS 1288 Section 4.

Nominate a thickness if:

* The glass is to be thicker than required by AS 1288 or applicable regulations.
* There are unusual conditions requiring detailed calculations for which the designer should be responsible.

In other cases the determination of thickness is usually within the competence of the glazing contractor.

Where thickness is determined by wind loading, the design wind pressure needs to be known in order to interpret the figures and tables of glass sizes and thicknesses in AS 1288.

Design wind pressure: To AS/NZS 1170.2 or AS 4055 as appropriate.

Materials and installation: To AS 1288.

Quality requirements for cut-to-size and processed glass: To AS/NZS 4667.

The standard specifies requirements for the following:

* Cut sizes of flat, clear ordinary annealed and tinted heat-absorbing glass with glossy, apparently plane and smooth surface, which are used for general and architectural glazing or similar.
* Cut sizes of flat, clear ordinary annealed and tinted heat-absorbing processing glass used for Grade A safety requirements (i.e. toughened or laminated).
* Cut sizes of ordinary annealed, patterned and wired glass used in decorative and general glazing applications.
* Cut sizes of wired glass used for Grade B safety and general glazing applications.
* Processed laminated and toughened glass.

### Manufacturer's documents

#### Technical manuals

Design, installation and operation manuals, CAD, BIM files and REVIT models: [www.safetylinejalousie.com.au/design-manual](http://www.safetylinejalousie.com.au/design-manual.shtml)

Contact Safetyline Jalousie for the latest product updates.

### Interpretation

#### Abbreviations

General: For the purposes of this worksection the following abbreviations apply:

* AGWA: Australian Glass and Window Association (formerly Australian Window Association (AWA)).
* WERS: Window Energy Rating Scheme.

Edit the **Abbreviations** subclause to suit the project or delete, if not required. List alphabetically.

#### Definitions

General: For the purposes of this worksection, the definitions given in AS/NZS 4668 and the following apply:

* Louvres - horizontal: Louvres that span horizontally between frame stiles, mullions or vertical supports.
* Total system SHGC: Solar heat gain coefficient as defined by the NCC and tested in conformance with NFRC 200.
* Total system U-Value: Thermal transmittance as defined by the NCC and tested in conformance with NFRC 100.

Edit the **Definitions** subclause to suit the project or delete if not required. List alphabetically.

### Submissions

#### Certification

Conformance: Submit evidence that the louvre windows conform to AS 2047.

Louvre window assemblies other than for housing may conform to AS 2047 clause 8.2 Labelling or AS 2047 clause 8.3 Certificate.

Protection of openable windows: Submit a certificate of on-site fall prevention testing.

On-site testing may not be required if type tests of window assemblies are available.

#### Operation and maintenance manual

General: Submit the Safetyline Jalousie instructions for operation, care and maintenance.

Refer to the Safetyline Jalousie website for care and maintenance details.

[www.safetylinejalousie.com.au/care-a-maintenance](http://www.safetylinejalousie.com.au/care-a-maintenance.html)

#### Products and materials

Type tests: Submit results as follows:

* Performance requirements, as documented.
* Protection of openable windows.

Type tests are carried out off-site. However, submission of evidence of a successful type test may be called up here for requirements specified in **SELECTIONS** or **PRODUCTS**, if there are no **SELECTIONS**.

Evidence of delivery: Submit delivery docket as evidence of delivery of

If evidence of delivery to site is required for particular products, consider including this *Optional* style text by changing to *Normal* style.

#### Samples

General: Submit samples of louvre window system components as follows:

* Manufacturer's standard hardware and accessories including louvre handles, anchor brackets and attachments, masonry anchors and weather seals (pile or extruded).
* Colour samples of prefinished production material showing the limits of the range of variation in the documented colour.
* Frame member profiles and louvre materials.
* Frame member joining techniques.

Glazing: Submit samples of glazing materials, each at least 200 x 200 mm, showing specified visual properties and the range of variation, if any, for each of the following types of glass:

* Tinted or coloured glass.
* Patterned or obscured glass or glazing plastics.

Edit as required.

Labelling: Label each sample with the series code reference and the date of manufacture.

#### Shop drawings

General: Submit shop drawings to a scale that best describes the detail, showing the following:

* Frame member profiles.
* Hardware, fittings and accessories including fixing details.

If louvre windows are to be fitted with non-standard hardware supplied by others, make sure that the selected louvre window suites can accept the selected hardware. Document hardware in the **SELECTIONS.**

* Junctions and trim to adjoining surfaces.
* Layout (sectional plan and elevation) of the window assembly.
* Lubrication requirements.
* Methods of installation including fixing, joint sealing and flashing.
* Provision for vertical and horizontal expansion.

#### Subcontractors

General: Submit names and contact details of proposed subcontractors endorsed by Safetyline Jalousie.

Evidence of experience:

Safetyline Jalousie have a fabricator network for supply and installation. Refer to the Safetyline Jalousie website.

Delete if supplier/installer details are not required.

#### Warranties

General: Submit warranties, as documented.

Describe the requirements of warranties in **PRODUCTS** or **EXECUTION**, as appropriate, and list the submissions required here.

### Inspection

#### Notice

Inspection: Give notice so that inspection may be made of the following:

* Openings prepared to receive windows (if windows are to be installed in prepared openings).
* Fabricated window assemblies at the factory ready for delivery to the site.
* Fabricated window assemblies delivered to the site, before installation.
* Commencement of window installation.
* Completion of window installation.

Amend to suit the project adding critical stage inspections required.

**Hold points**, if required, should be inserted here.

## Products

### General

#### Product substitution

Other products: Conform to PRODUCTS, **GENERAL**, **Substitutions** in *0171 General requirements*.

The *0171 General requirements* clause sets out the submissions required if the contractor proposes alternative products. Refer also to NATSPEC TECHnote GEN 006 for more information on proprietary specification.

#### Storage and handling

Storage: Store in a clean, dry area and unaffected by weather, to the manufacturer's recommendations. Protect from building materials and loose debris such as wet plaster, mortar, paint and welding splatter.

#### Acoustic performance

Louvre windows: Tested to AS 5218.

#### Protection of openable windows

Fall prevention: To BCA D2.24 and BCA 3.9.2.

Testing: To AS 5203.

Windows supplied as complete sets with security grilles and tested to AS 5041 are not required to be tested to AS 5203.

#### Marking

Louvre window assemblies: To AS 2047 Section 8.

Louvre window assemblies other than for housing may conform to AS 2047 clause 8.2 Labelling or AS 2047 clause 8.3 Certificate.

#### Product identification

General: Marked to show the following:

* Manufacturer’s identification.
* Product brand name.
* Product type.
* Quantity.
* Product reference code and batch number.
* Date of manufacture.

Edit the list to suit the project or delete if not required.

### Glass

#### Glazing

Glass type:

Refer to the Safetyline Jalousie website and select from the range of Clear, Tinted, Low-E and Satin glass.

Thickness: 6, 6.38 or 6.5 mm annealed, laminated, toughened or toughened and heat soak tested or 6.5 mm vacuum glazed.

#### Safety glass

Standard: To AS/NZS 2208.

AS/NZS 2208 includes toughened, laminated, wired, organic-coated glass and safety glazing plastics. See AS 1288 Section 5 for the required grade (A or B) for each application.

Certification: Required.

* Certification provider: An organisation accredited by the Joint Accreditation System of Australia and New Zealand (JAS-ANZ).

### Glass identification

#### Safety glazing materials

Identification: Identify each piece or panel, to AS 1288.

Identification: See AS 1288 clause 5.23.

### Glazing materials

If windows and glazed doors are selected as complete proprietary items, delete this clause.

#### General

Requirement: Glazing materials (including putty, glazing compounds, sealants, gaskets, glazing tapes, spacing strips, spacing tapes, spacers, setting blocks and compression wedges appropriate for the conditions of application and required performance.

#### Jointing materials

Requirement: Provide jointing and pointing materials to manufacturer's recommendations that are compatible with each other and the contact surfaces and non-staining to finished surfaces. Do not provide bituminous materials on absorbent surfaces.

#### Elastomeric sealants

Sealing compound (polyurethane, polysulfide, acrylic): To ASTM C920 or ISO 11600.

Sealing compound (silicone): To ASTM C920 or ISO 11600.

Sealing compound (butyl): To ASTM C1311.

### Louvre window assemblies

#### General

Description: Louvre blades mounted in a metal surround frame or subframe and able to withstand the permissible-stress-design wind pressure for that location without failure or permanent distortion of members, and without louvre blade flutter.

#### Adjustable louvres

Description: Louvre blades glazed into louvre bearers, and end caps linked into bars, attached to side jamb together in banks. Each bank is operated by an individual operating handle.

Safetyline Jalousie louvres open completely to the outside, opening up to 80° with no interference to blinds and curtains with four different locking positions (three open and one closed) with the standard lever. Other operators are available which provide differing opening variants.

Select from the following Safetyline Jalousie louvre window products and nominate here:

* Glass louvre blades: Mounted in an aluminium blade holder (louvre bearer), fixed on three sides of the blade and hinged at the rear edge of each blade holder at 135 mm centres to the fixed window frame.
* Aluminium louvre blades: Curved 135 mm wide (one piece) blades hinged at the rear edge to the fixed window frame at 135 mm centres.

Seals:

Nominate here type and extent of seals to be provided.

Safetyline Jalousie louvre blades are sealed on all four sides with EPDM gaskets.

Operating handles:

The number required per window is dependent on the louvre type and width, refer to the manufacturer’s recommendations for the number of operators required. Delete if requirement is more appropriately covered in **SELECTIONS, Louvre window schedule.**

#### Power operated louvres

Description: Louvres with automated operating mechanisms to suit louvre size operated with or without remote control.

Louvre controls may be integrated with a building management system.

### Insect screens

Insect screens are usually installed to the external face of frame. Make sure the louvre assembly is located so that when fully opened the louvre blades are clear of the insect screens and security grille.

#### Fixed screens

General: Fixed screens fitted to the window frames with a clipping device that permits removal for cleaning.

#### Retractable screens

General: Proprietary retractable insect screen comprising aluminium frame and fibreglass mesh, fitted between the guide channels incorporated in the frame, and a retraction system including tension spring, nylon bearings, positive self-locking device, and plastic sealing strip at sill.

#### Aluminium framed screens

General: Aluminium extruded sections with mesh fixing channel, mitred, staked and screwed at corners.

Mesh: Bead the mesh into the frame channel with a continuous resilient gasket, so that the mesh is taut and free of distortion.

Safetyline Jalousie provides fixed insect screens attached to the inside of window frames, these screens may be removed for cleaning. Select from the following mesh types:

* Aluminium.
* Stainless steel.
* Fibreglass.

### Security window grilles

#### General

Requirement: Provide proprietary metal security grilles or operable screen and frame, fixed to the building structure with tamper resistant fastenings.

Security rods: Optional 8 mm diameter stainless steel rods inserted into the louvre blade holder.

Security window grilles: To AS 5039.

AS 5039 acknowledges that the security window grilles described are not intruder proof. See the foreword to this standard. The dynamic impact, knifeshear, jemmy, pull and shear tests scheduled for compliance in AS 5039, Table 1 or described in AS 5041.

### Aluminium frame finishes

Delete finish not required.

#### Powder coatings

Standard: To AS 3715.

Product:

Product: e.g. AkzoNobel Interpon or Dulux standard powder coatings.

Type: 7 year or 10 year warranty coatings from Interpon and Dulux.

AS 3715 sets minimum standards for various performance criteria. Consult with manufacturers if variations are proposed.

AkzoNobel Interpon and Dulux offer powder coatings with enhanced protection that carry 10 year, 15 year and 20 year warranties.

Edit as appropriate.

Colour:

Nominate colour name and code from AkzoNobel Interpon or Dulux powder coatings colour charts

#### Anodised

Standard: To AS 1231.

Thickness: 20 or 25 microns.

25 micron thick anodising, recommended for severe industrial and coastal conditions, can be made available by some suppliers upon request.

Colour:

Select from the available range of colours by Australian Aluminium Finishing (AAF) or Universal Anodisers.

### Ancillary components and fittings

#### Fasteners

Requirement:

Comply with the louvre window manufacturer’s recommendations and AS 2047 (for residential and commercial building) and AS 4055 (for houses) for fastener requirements.

Allow for the following requirements to suit fixing substrate:

* For aluminium – use aluminium or 300 series stainless steel fasteners.
* For galvanized steel – use hot-dipped galvanized steel or 300 series stainless steel fasteners.
* For stainless steel – use 300 series stainless steel fasteners.

Size and type: To suit louvre window unit size and wind loading conditions.

#### Flashings

General: Corrosion resistant, compatible with the other materials in the installation, and coated with a non-staining compound where necessary.

Standard: To AS/NZS 2904.

#### Extruded gaskets and seals

General: Provide seals, as documented.

Type: Non-cellular (solid) elastopressive seals.

Location or function:

Material:

* Rubber products (neoprene, ethylene propylene diene monomer (EPDM) or silicone rubber): To BS 4255-1.
* Flexible polyvinyl chloride (PVC): To BS 2571, E type compounds, colour fastness grade B.

#### Pile weather strips

Standard: To AAMA 701/702.

Standard: AAMA 701/702 is a guide to selecting pile weather strips used in windows and doors. It defines requirements to restrict air and water penetration.

Location:

Materials: Polypropylene or equivalent pile and backing, low friction silicone treated, ultra violet stabilised.

## Execution

### Pre-installation

#### General

Timber reveals: Prime all surfaces of timber reveals which are to be painted before fixing to aluminium frames.

### Installation

#### Glazing

General: Install the glass as follows:

* Permanently fix in place each piece of glass to withstand the normal loadings and ambient conditions at its location without distortion or damage to glass and glazing materials.
* No transfer of building movements to the glass.
* Watertight and airtight for external glazing.

Temporary marking: Use a method which does not damage the glass. Remove marking on completion.

Toughened glass: Do not cut, work, or permanently mark after toughening. Use installation methods which prevent the glass making direct contact with metals or other non-resilient materials.

Heat absorbing glass: Provide wheel cut edges without damage or blemishes and with minimum feather in locations exposed to direct sunlight.

#### Louvre windows

General: Install louvre windows frames as follows:

* Plumb, level, straight and true within building tolerances.
* Fixed or anchored to the building structure in conformance with the wind action loading.
* Isolated from any building loads, including loads caused by structural deflection or shortening.
* Allow for thermal movement.

Power operated louvre windows: Make sure power and control signal services are provided at the louvre controls.

#### Weatherproofing

Flashing and weatherings: Install flashings, weather bars, drips, storm moulds, joint sealant and pointing to prevent water penetrating the building between the window frame and the building structure under the prevailing service conditions, including normal structural movement of the building.

#### Fixing

General: Do not penetrate metal flashings with fixings.

Packing: Pack behind fixing points with durable full width packing.

Fastener spacing (nominal): 600 mm and maximum 150 mm from reveal ends.

Fasteners: Conceal fasteners. Use size and type to suit window unit size and wind loading conditions.

#### Joints

Requirement: Make accurately fitted tight joints so that fasteners and fixing devices such as pins, screws, adhesives and pressure indentations are not visible on exposed surfaces.

Sealants:

* If priming is recommended, prime surfaces in contact with jointing materials.
* If frames are powder coated, apply a neutral cure sealant.

#### Operation

General: Make sure moving parts operate freely and smoothly, without binding or sticking, at correct tensions or operating forces and are lubricated.

#### Protection

Removal: Remove temporary protection measures from the following:

* Contact mating surfaces before joining up.
* Exposed surfaces.

Temporary measures:

State a particular method here, or delete to leave the choice of method to the contractor. For on-site care see AS 2047 – Appendix E (Informative).

#### Trim

General: Provide mouldings, architraves, reveal linings, and other internal trims using materials and finishes matching the window frames. Make neat and clean junctions between frames and the adjoining building surfaces.

### Security window grilles

#### General

Installation: To AS 5040.

### Completion

#### Repair of finish

Polyester or fluoropolymer coatings: Contact supplier for approval to apply touch up products, otherwise replace damaged material.

#### Cleaning

Method: Clean with soft clean cloths and clean water, finishing with a clean squeegee. Do not use abrasive or alkaline materials.

Extent: All frames and glass surfaces inside and out.

#### Warranties

Louvre windows: Provide the manufacturer's published product warranties.

Use only where warranties extending beyond the defects liability period are available for the particular system. Insert the required warranty period and terms, which should be negotiated beforehand. If the warranty is in the form of separate material and installation warranties, require the signatures of both manufacturer and installer. If documenting warranties change the following Optional style text to Normal style text:

Warranty: Provide a warranty on
Form of warranty:
Minimum period:
Powder coating:
Hardware:

The form(s) required should be provided as part of the contract documentation.

Form of warranty: e.g. Against failure of materials and operation under normal environment and use conditions.

Minimum period: e.g. As offered by the manufacturer. Safetyline Jalousie provides a 6 year warranty for the materials and workmanship of its products. Full details can be found at the Safetyline Jalousie website.

Powder coating: e.g. As offered by the manufacturer for the selected finish.

Hardware: e.g. As offered by the manufacturer.

## Selections

**Schedules** are a way of documenting a selection of proprietary or generic products or systems by their properties. Indicate their locations here and/or on the drawings. Refer to NATSPEC TECHnote GEN 024 for guidance on using and editing schedules.

### Performance

#### Louvre window performance schedule

| Property | A | B | C |
| --- | --- | --- | --- |
| Total system U-Value (W/m2 .K) |  |  |  |
| Total system SHGC |  |  |  |
| Weighted sound reduction index (Rw and Rw  + Ctr) |  |  |  |
| Visible transmittance (Tvis) |  |  |  |
| Reflectance (%) |  |  |  |
| WERS Energy rating%: Heating |  |  |  |
| WERS Energy rating%: Cooling |  |  |  |
| AGWA Compliance Certificate |  |  |  |
| Water penetration resistance (Pa) |  |  |  |
| Fire-resistance level (FRL) |  |  |  |
| Ultimate limit state (ULS) wind pressure (Pa) |  |  |  |
| Serviceability limit state (SLS) wind pressure (Pa) |  |  |  |
| Openable (free) area (m2) |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Total system U-Value (W/m2.K): Insert the thermal transmittance value used for determining NCC compliance. These should be obtained from tests to NFRC 100. Select the product to fulfil design and compliance requirements. See NATSPEC TECHnote DES 015 on BCA Energy efficiency.

Total system SHGC: Insert the solar heat gain coefficient value used for determining NCC compliance. These should be obtained from tests to NFRC 200. Select the product to fulfil design and compliance requirements.

Weighted sound reduction index: State the required rating to AS/NZS ISO 717.1. It is advisable to obtain the advice of an acoustic consultant on the selection of a Rw or Rw  + Ctr rating for sound transmission reduction. Refer to NATSPEC TECHnote DES 032 for information on airborne sound insulation.

Visible transmittance (Tvis): The visible light passing directly through the glass. The higher the Tvis, the more daylight.

Reflectance %: A maximum value is often a council requirement. Refer to the ABCB Glazing calculator [www.abcb.gov.au](https://www.abcb.gov.au/Resources/All-Resources?types=%7bBBD8390F-884A-4FE4-BD0B-C52AF4A0989A%7d). Delete if this requirement is more appropriately covered in the **Glass schedule**.

WERS Energy rating: Star rating system operated by the Australian Window Association.

AGWA Certificate of Compliance: Insert Required or Not required. The AGWA (formerly AWA) Compliance Certificate will cover only those products that conform to AS 2047.

Water penetration resistance: e.g. 150 Pa.

Fire-resistance level (FRL): State the required level to AS 1530.4, delete or state Not applicable. See NATSPEC TECHnote DES 020 on fire behaviour of building materials and assemblies.

Ultimate and serviceability design wind pressure: Nominate the design wind pressures for the project to AS/NZS 1170.2 (for residential and commercial building) or AS 4055 (for housing, Class 1 and 10a buildings). AS 2047 Appendix A includes an informative guide to design wind pressure.

Openable area: State the openable area in m2 to achieve NCC requirements for natural ventilation.

### Louvre windows

#### Louvre window schedule

For a summary and comparison of Safetyline Jalousie window systems and guidance on selecting Safetyline Jalousie louvre window options, refer to the Safetyline Jalousie website.

| Property | A | B | C |
| --- | --- | --- | --- |
| Product name |  |  |  |
| Proprietary suite |  |  |  |
| Frame material |  |  |  |
| Frame finish |  |  |  |
| Louvre blade material |  |  |  |
| Louvre blade finish |  |  |  |
| Louvre window height and blade length (mm) |  |  |  |
| Operator type |  |  |  |
| Security bars |  |  |  |
| Controls |  |  |  |
| Screen: Frame material and finish |  |  |  |
| Screen: Mesh type |  |  |  |
| Glazing |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Product name: e.g. Safetyline Jalousie louvre windows.

Proprietary suite: e.g. JX Louvre Window with 63 mm extruded aluminium frame.

Frame material: e.g. Aluminium.

Frame finish: e.g. Powder coated, high performance powder coated, anodised.

Louvre blade material: e.g. Curved aluminium, glass. See *Guidance* on **Glazing** below.

Louvre blade finish: e.g. Powder coated, High performance powder coated, Anodised. See *Guidance* on glazing below.

Louvre window height and blade length: Refer to Safetyline Jalousie Standard Heights – Glass Louvres, Standard Heights – Aluminium Louvres tables. Alternative: Note sizes on drawings.

Operator type: e.g. Left Lever, Right Lever, Reversible Turn Handle, Turn Handle. Delete if requirement is more appropriately covered in **PRODUCTS.**

Security bars: Yes/no. Include details of material and finish, e.g. stainless steel.

Controls: e.g. Lever, Winder.

Screen:

* Frame material: Aluminium, Timber or PVC-U.
* Frame finish: Powder coat, Anodised, Paint, Clear finish, No applied finish.
* Mesh type: e.g. Coated aluminium, Fibreglass, Corrosion resistant steel or Bronze.
* Bushfire protection: BCA 3.10.5 and AS 3959 call for screens of aluminium, corrosion resistant steel or bronze with a maximum aperture size of 2 mm to areas of medium bushfire attack category and excludes aluminium mesh in areas of high category. Fibreglass mesh is excluded in all bushfire areas.lternatively document screens in the **Screen schedule** and bushfire shutters in *0457 External screens.*

Glazing: Document the glazing type and thickness in this schedule or the **GLAZING,** **Glass schedule**. Specifying glazing in this schedule is suitable for projects where the same glass is used for each window or glazed door type. It can be documented by description, e.g. 6.38 mm clear laminated glass, or by reference to a designated glass type in the **Glass schedule**. The latter approach may be more appropriate for projects with a large number of glazing types, or glazing that requires more detailed specification.

Safetyline Jalousie can provide any Viridian glass, providing the thickness is either 6 mm or 6.38 mm.

Refer to the *Guidance* for **Glass schedules** and the NATSPEC TECHnote PRO 006 for guidance on glass types.

For protection of openable windows, document a device to restrict the window opening in this schedule**,** a screen in the **Screen schedule** and a barrier, as required.

#### Power operated louvre window schedule

For a summary and comparison of Safetyline Jalousie window systems and guidance on selecting Safetyline Jalousie louvre window options, refer to the Safetyline Jalousie website.

| Property | A | B | C |
| --- | --- | --- | --- |
| Product name |  |  |  |
| Proprietary suite |  |  |  |
| Frame material |  |  |  |
| Frame finish |  |  |  |
| Motor mounting |  |  |  |
| Louvre blade material |  |  |  |
| Louvre blade finish |  |  |  |
| Louvre window height and blade length (mm) |  |  |  |
| Number of Banks |  |  |  |
| Operation/control |  |  |  |
| Security bars |  |  |  |
| Insect screen: Frame material and finish |  |  |  |
| Insect screen: Mesh type |  |  |  |
| Glazing |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Product name: e.g. Safetyline Jalousie louvre windows.

Proprietary suite: e.g. JX Louvre Window with 63 mm extruded aluminium frame.

Frame material: e.g. Aluminium.

Frame finish: e.g. Powder coated, high performance powder coated, anodised.

Motor mounting: e.g. Externally mounted on the frame or Concealed within the frame.

Louvre blade material: e.g. Curved aluminium, glass. See *Guidance* on glazing below.

Louvre blade finish: e.g. Powder coated, High performance powder coated, Anodised. See *Guidance* on glazing below.

Louvre window height and blade length: e.g. Blade height of 135 mm. Refer to Safetyline Jalousie Standard Heights – Glass Louvres, Standard Heights – Aluminium Louvres tables. Alternative: Note sizes on drawings.

Number of Banks: Refer to Safetyline Jalousie Standard Heights – Glass Louvres, Standard Heights – Aluminium Louvres tables. Alternative: Indicate number on drawings.

Operation/control: e.g. Wall switches, remote controls, control by sensor, integration with building management systems (central building control panel).

Security bars: Yes/no. Include details of material and finish, e.g. stainless steel.

Insect screen: Frame material and finish:

* Frame material: Aluminium, Timber or PVC-U.
* Frame finish: Powder coat, Anodised, Paint, Clear finish, No applied finish.

Insect screen: Mesh type: e.g. Coated aluminium, Fibreglass, Corrosion resistant steel or Bronze. BCA 3.10.5 and AS 3959 call for screens of aluminium, corrosion resistant steel or bronze with a maximum aperture size of 2 mm to areas of medium bush fire attack category and excludes aluminium mesh in areas of high category. Fibreglass mesh is excluded in all bush fire areas.

Glazing: Document the glazing type and thickness in this schedule or the **GLAZING,** **Glass schedule**. Documenting glazing in this schedule is suitable for projects where the same glass is used for each window. It can be documented by description, e.g. 6.38 mm clear laminated glass, or by reference to a designated glass type in the **Glass schedule**. The latter approach may be more appropriate for projects with a large number of glazing types, or glazing that requires more detailed specification.

Safetyline Jalousie can provide any Viridian glass, providing the thickness is either 6 mm or 6.38 mm.

Refer to the *Guidance* for **Glass schedules** and the NATSPEC TECHnote PRO 006 for guidance on glass types.

For protection of openable windows, document a device to restrict the window opening in this schedule, a screen in the **Screen schedule** and a barrier, as required.

### Screens

#### Screen schedule

| Property | A | B | C |
| --- | --- | --- | --- |
| Product name |  |  |  |
| Generic description |  |  |  |
| Frame material |  |  |  |
| Frame finish |  |  |  |
| Mesh type |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Product name: Safetyline Jalousie louvre windows.

Generic description: e.g. Flyscreen, Fire protection screen, Fall prevention screen or Bushfire screen. See the security window grille schedule for security grilles. See BCA D2.24 and BCA 3.9.2 for openable windows requiring fall prevention devices, screens and barriers.

Frame material: e.g. Aluminium.

Frame finish: e.g. Powder coat, Anodised.

Mesh type: e.g. Aluminium, Fibreglass, or Stainless steel.

Bushfire protection: See construction requirements in AS 3959 for the relevant BAL. BCA 3.10.5 and AS 3959 call for screens of aluminium, corrosion resistant steel or bronze with a maximum aperture size of 2 mm to areas of medium bush fire attack category and excludes aluminium mesh in areas of high category. Fibreglass mesh is excluded in all bushfire areas. Alternatively document screens in the **Louvre window schedule** and bushfire shutters in *0457 External screens.*

### Security window grilles

#### Security window grille schedule

| Property | A | B | C |
| --- | --- | --- | --- |
| Product name |  |  |  |
| Generic description |  |  |  |
| Material |  |  |  |
| Finish |  |  |  |
| Hinge: Material |  |  |  |
| Hinge: Fixing |  |  |  |
| Hardware |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Product name: Delete if the selection is by generic performance.

Generic description: AS 5039 clause 5.2 describes the three window screen security classification type as follows.

* Type I prevents an arm from passing through.
* Type II allows an arm but prevents bodily entry.
* Type III prevents insects passing through.

Material: Steel, Stainless steel or Aluminium.

Finish: See AS 5039 clause 6.2 for corrosion protection finishes.

Hinges:

* Material: e.g. Aluminium, stainless steel or steel.
* Fixing: Rivets or fastening devices. See AS 5039 clauses 6.7, and 6.8.

Hardware: See AS 5039 clause 6.5. If the manufacturer’s standard lock and hardware are not acceptable, nominate hardware to comply. Coordinate with your hardware schedule.

### Glazing

#### Glass schedule

| Property | A | B | C |
| --- | --- | --- | --- |
| Glass type |  |  |  |
| Glass thickness (mm) |  |  |  |
| Body tint colour |  |  |  |
| Interlayer colour |  |  |  |
| Surface coating |  |  |  |
| Surface coating: Colour |  |  |  |
| Reflective coating: Colour |  |  |  |
| Reflective coating: % reflectance |  |  |  |
| Surface pattern |  |  |  |
| Surface processing |  |  |  |
| Surface processing: Pattern |  |  |  |
| Surface processing: Colour |  |  |  |
| Edge processing |  |  |  |
| Number of edges processed |  |  |  |

A, B, C: These designate each instance or type or location of the item scheduled.

Edit codes in the **Schedule** to match those on drawings.

Glass type: Refer to NATSPEC TECHnote PRO 006 for guidance on glass types.

Glass thickness: It is generally not necessary to document thickness. Nominate a thickness where:

* The glass is to be thicker than required by AS 1288 or applicable regulations.
* There are unusual conditions requiring detailed calculations for which the designer should be responsible.

In other cases, the determination of thickness is usually within the competence of the glazing contractor.

Body tint colour: e.g. Grey, Bronze, Green, Blue. Consult the manufacturer for colours available. Do not use body tinted wired (cast or polished) in locations exposed to the sun; fracture may result.

Interlayer colour: For laminated glasses only. Consult the manufacturer for the colours available.

Surface coating: Describe by coating function, e.g. Solar control, Low emission, Self-cleaning, Decorative or by coating type, e.g. pyrolitic hard coating, vacuum sputtered or ceramic. Coatings are best described by the manufacturer’s brand name.

* Self-cleaning: Glass incorporating a coating which dissolves dirt (photo activ) and sheds water (hydrophilic) using natural UV light and rain.

Surface coating: Colour: e.g. Grey, Bronze, Green, Blue. Consult the manufacturer for colours available.

Reflective coating: Colour: e.g. silver, gold, bronze. Consult the manufacturer for colours available. Reflective coatings may be available on either clear or body tinted float. Consult manufacturer.

Reflective coating: % reflectance: Consult the manufacturer for reflectances available. Delete if this requirement is more appropriately covered in the **Louvre window performance schedule**.

The manufacturer’s brand name is often the best way to identify tinted, reflective, and patterned glasses.

Surface pattern: For patterned glass only. Proprietary patterns are best described by the manufacturer’s brand name. Patterns include diffuse reflection (picture glass).

Surface processing: e.g. Screen printing with ceramic paint fused to the surface, Sandblasting, Acid etching.

Surface processing: Pattern: Proprietary patterns are best described by the manufacturer’s brand name.

Surface processing: Colour: Applicable to screen printed patterns only.

Edge processing: Maximum width varies with thickness. Wired glass is restricted to rough arrised edges. Consult with processor. Common edge types and typical applications for each edge type are:

* None (clean cut, no processing).
* Flat ground: Silicone structural glazing with exposed edges.
* Flat polished: Silicone structural glazing where edge condition is critical for aesthetic purposes
* Ground pencil edge: Mirrors, decorative furniture glass.
* Polished pencil edge: Mirrors, decorative furniture glass.
* Ground mitre: Silicone structural glazing.
* Bevelled: Mirrors, decorative furniture glass.
* Seamed edges: Normal edge treatment for heat-treated glass.

Refer also to NATSPEC TECHnote PRO 006 for more information on this topic.

Number of edges processed: e.g. 1 long, 2 long, All.

REFERENCED DOCUMENTS

**The following documents are incorporated into this worksection by reference:**

AS 1231 2000 Aluminium and aluminium alloys - Anodic oxidation coatings

AS 1288 2006 Glass in buildings - Selection and installation

AS 2047 2014 Windows and external glazed doors in buildings

AS/NZS 2208 1996 Safety glazing materials in buildings

AS/NZS 2904 1995 Damp-proof courses and flashings

AS 3715 2002 Metal finishing - Thermoset powder coating for architectural applications of aluminium and aluminium alloys

AS/NZS 4667 2000 Quality requirements for cut-to-size and processed glass

AS/NZS 4668 2000 Glossary of terms used in the glass and glazing industry

AS 5039 2008 Security screen doors and security window grilles

AS 5040 2003 Installation of security screen doors and window grilles

AS 5203 2016 Protection of openable windows/ fall prevention – Test sequence and compliance method

AS 5218 2018 Acoustic performance of windows and doors - Methods of test

BCA 3.9.2 2019 Acceptable construction - Safe movement and access - Barriers and handrails

BCA D2.24 2019 Access and egress - Construction of exits - Protection of openable windows

BS 2571 1990 Specification for general-purpose flexible PVC compounds for moulding and extrusion

BS 4255 Rubber used in preformed gaskets for weather exclusion from buildings

BS 4255-1 1986 Specification for non-cellular gaskets

AAMA 701/702 2011 Voluntary specification for pile weatherstripping and replaceable fenestration weatherseals

NFRC 100 2020 Procedure for determining fenestration product U-factors

NFRC 200 2020 Procedure for determining fenestration product solar heat gain coefficient and visible transmittance at normal incidence

**The following documents are mentioned only in the *Guidance* text:**

AS ISO 717 Acoustics - Rating of sound insulation in buildings and of building elements

AS/NZS ISO 717.1 2004 Airborne sound insulation

AS/NZS 1170 Structural design actions

AS/NZS 1170.2 2011 Wind actions

AS 1530 Methods for fire tests on building materials, components and structures

AS 1530.4 2014 Fire-resistance tests for elements of construction

AS 3959 2018 Construction of buildings in bushfire-prone areas

AS 4055 2012 Wind loads for housing

AS 5041 2003 Methods of test - Security screen doors and window grilles

BCA 3.10.5 2019 Acceptable construction - Ancillary provisions and additional construction requirements - Construction in bushfire prone areas

NATSPEC DES 015 2019 NCC - BCA Volume One Energy efficiency provisions

NATSPEC DES 020 2018 Fire behaviour of building materials and assemblies

NATSPEC DES 032 2018 Airborne sound insulation

NATSPEC GEN 006 2015 Product specifying and substitution

NATSPEC GEN 024 2019 Using NATSPEC selections schedules

NATSPEC PRO 006 2016 Glass types used in buildings

NATSPEC TR 01 2019 Specifying ESD